Braket comes moved to where it doesnt clip, if you like it where it is follow 1-4 if you want to move it follow 1-7

1. First import KLE0's Havis tablet and move the tablet in "PUT TABLET IN HERE" dummy
2. Then under display - local axes press the arrow and un tick "keep object"
3. Then press "Reset to Parent" and click the bracket mesh
4. Then attach KLE0's Havis tablet to the bracket.
5. To adjust the bracket first move the bracket part with piviot off in top view to get left right rotation.
6. To get up down movement first attach the bracket to the hinge and with piviot off in left or right view to get up down rotation.
7. Lastly attach the hinge to the base.

To be used with KLE0's Havis tablet

Fitted to GMS FPIS