1. First attach KLE0's Havis tablet to the bracket.
2. To adjust the bracket first move the bracket part with piviot off in top view to get left right rotation.
3. To get up down movement first attach the bracket to the hinge and with piviot off in left or right view to get up down rotation.
4. Lastly attach the hinge to the base.

To be used with KLE0's Havis tablet

Fitted to GMS PPV tahoe, can be used on his SSV just need to move it if needed